Avaya Client Services API Reference (iOS)

- Main Page
- Classes
- Files
- Related Pages

- File List
- File Members

Enumerations
CSFeatureType.h File Reference
`#import <Foundation/Foundation.h>`

## Enumerations
enum | CSFeatureType { CSFeatureTypeUninitialized = 0, CSFeatureTypeSendAllCalls, CSFeatureTypeForwardAllCalls, CSFeatureTypeForwardBusyNoAnswerCalls, CSFeatureTypeExclusion, CSFeatureTypeEC500, CSFeatureTypeExtendCall, CSFeatureTypeCallPark, CSFeatureTypeCallUnpark, CSFeatureTypeAutoCallback, CSFeatureTypeWhisperPage, CSFeatureTypeGroupCallPickup, CSFeatureTypeExtendedGroupCallPickup, CSFeatureTypeCallingPartyNumberBlock, CSFeatureTypeCallingPartyNumberUnblock, CSFeatureTypeOneTouchRecording, CSFeatureTypeDirectedCallPickup, CSFeatureTypePriorityCall, CSFeatureTypeEnhancedCallForwarding, CSFeatureTypeBusyIndicator, CSFeatureTypeAutodial, CSFeatureTypeHuntGroupBusyPosition, CSFeatureTypeTeamButton, CSFeatureTypeMaliciousCallTrace, CSFeatureTypeNoHoldConference, CSFeatureTypeLimitCalls, CSFeatureTypeServiceObserving, CSFeatureTypeForwardBusyCall, CSFeatureTypeForwardNoAnswerCalls, CSFeatureTypeForwardNumber, CSFeatureTypeForwardBusyNumber, CSFeatureTypeAutoConference, CSFeatureTypeCancelAllForwarding, CSFeatureTypeForwardToVoiceMail, CSFeatureTypeStationLogout, CSFeatureTypeDirectDial, CSFeatureTypeMoveCall, CSFeatureTypeRetrieveCall, CSFeatureTypeInternalTwinning, CSFeatureTypeSimRingCallback, CSFeatureTypeCallbackCall, CSFeatureTypeSendNN }
| Defines the list of supported features. More...

## Enumeration Type Documentation

enum CSFeatureType

Defines the list of supported features.

This enum is for all of the features supported by the signaling engine, not tailored based on capabilities provisioned for the user in the network. It is also not tailored based on which features are client invokable via -[CSUser invokeFeature:].

Enumerator
CSFeatureTypeUninitialized | The uninitialized (or unknown) feature type.
CSFeatureTypeSendAllCalls | Send All Calls is an AST-I feature that uses a 'Feature-Named-URI' (FNU) that is used to activate/deactivate coverage path for calls coming in at a CM station (extension). In summary, the feature activates/de-activates call coverage at CM. Depending on how CM extension is provisioned, the calls may be covered to another extension, voice mail, etc. Incoming priority calls are not affected by the feature's status, that is, incoming priority calls do not get covered as a result of activating the SAC feature. It should be noted that the SAC feature FNU may be used to apply to local user's CM extension as well as to a third party CM extension (avaya-cm-destination).
CSFeatureTypeForwardAllCalls | Call Forward All is an AST-I feature that uses a 'Feature-Named-URI' (FNU) that is used to activate/deactivate call forwarding for calls coming in at a CM station (extension). In summary, the feature activates/de-activates call forwarding at CM. It should be noted that the call forward all feature FNU may be used to apply to local user's CM extension as well as to a third party CM extension (avaya-cm-destination).
CSFeatureTypeForwardBusyNoAnswerCalls | Call Forward Busy No Answer is an AST-I feature that uses a 'Feature-Named-URI' (FNU) that is used to activate/deactivate call forwarding for incoming calls when busy or when not answered by the user at a CM station (extension). In summary, the feature activates/de-activates call forwarding at CM. It should be noted that this feature FNU may be used to apply to local user's CM extension as well as to a third party CM extension (avaya-cm-destination).
CSFeatureTypeExclusion | Exclusion is an AST-I feature that uses a 'Feature-Named-URI' (FNU) that is used to activate/deactivate exclusion by a bridged line appearance user. In summary, the feature activates/de-activates exclusion at the CM station associated with the user.
CSFeatureTypeEC500 | EC500 is an AST-I feature that uses a 'Feature-Named-URI' (FNU) that is used to activate/deactivate EC 500 cellular call extension at a CM station (extension). In summary, the feature activates/de-activates EC500 feature at CM station.
CSFeatureTypeExtendCall | Extend Call is an AST-I feature that uses a 'Feature-Named-URI' (FNU) that is used to extend a call to the off-PBX destinations associated with the extension. In summary, the feature invokes extend call at the CM station associated with the user.
CSFeatureTypeCallPark | Call Park is an AST-I feature that uses a 'Feature-Named-URI' (FNU) that allows the user to place the current call in the call park state so it can be retrieved from another phone. In summary, the feature invokes call park at the CM station associated with the user.
CSFeatureTypeCallUnpark | Call Unpark is an AST-I feature that uses a 'Feature-Named-URI' (FNU) that allows the user to retrieve a call parked at another extension. In summary, the feature invokes call unpark at the CM station associated with the user.
CSFeatureTypeAutoCallback | Auto Callback is an AST-I feature that uses a 'Feature-Named-URI' (FNU) that allows a user who placed a call to a busy or unanswered telephone to be called back automatically when the called telephone becomes available to receive a call. In summary, the feature activates/de-activates auto-callback at the CM station associated with the user.
CSFeatureTypeWhisperPage | Whisper Page is an AST-I feature that uses a 'Feature-Named-URI' (FNU) that allows the user to to make and receive whisper pages. A whisper page is an announcement sent to another extension that is active on a call where only the person on the extension hears the announcement; any other parties on the call cannot hear the announcement. In summary, the feature activates/de-activates whisper page at the CM station associated with the user.
CSFeatureTypeGroupCallPickup | Group Call Pickup is an AST-I feature that uses a 'Feature-Named-URI' (FNU) that allows the user to answer a call that is ringing in the user's pickup group. In summary, the feature invokes group call pickup at the CM station associated with the user.
CSFeatureTypeExtendedGroupCallPickup | Extended Group Call Pickup is an AST-I feature that uses a 'Feature-Named-URI' (FNU) that allows a user to answer calls directed to another call pickup group. In summary, the feature invokes extended group call pickup at the CM station associated with the user.
CSFeatureTypeCallingPartyNumberBlock | Calling Party Number Block is an AST-I feature that uses a 'Feature-Named-URI' (FNU) that allows a user to block the sending of the calling party number for one call. In summary, the feature invokes calling party number block at the CM station associated with the user.
CSFeatureTypeCallingPartyNumberUnblock | Calling Party Number Unblock is an AST-I feature that uses a 'Feature-Named-URI' (FNU) that allows a user to deactivate calling party number (CSN) blocking and allows the CSN to be sent for a single call. In summary, the feature invokes calling party number unblock at the CM station associated with the user.
CSFeatureTypeOneTouchRecording | One-Touch Recording is an AST-I feature that uses a 'Feature-Named-URI' (FNU) that allows a user to start and end the recording of an in-progress conversation using the AUDIX system recording facility. In summary, the feature invokes one-touch recording at the CM station associated with the user.
CSFeatureTypeDirectedCallPickup | Directed Call Pickup is an AST-I feature that uses a 'Feature-Named-URI' (FNU) that allows the user to answer a call ringing at another extension without having to be a member of a pickup group. In summary, the feature invokes directed call pickup at the CM station associated with the user.
CSFeatureTypePriorityCall | Priority Call is an AST-I feature that uses a 'Feature-Named-URI' (FNU) that allows a user to place priority calls or change an existing call to a priority call. In summary, the feature invokes priority call at the CM station associated with the user.
CSFeatureTypeEnhancedCallForwarding | Enhanced Call Forwarding is feature that uses a 'Feature-Named-URI' (FNU) that allows a user to configure call forwarding for internal or external calls with seprate settings for busy, no reply, and unconditional forwarding. In summary, the feature invokes enhanced call forwarding at the CM station associated with the user.
CSFeatureTypeBusyIndicator | Busy Indicator is a feature that allows one to observe another extension for its availability. When the far end destination goes off-hook, CM notifies the same via <feature name ="busy-indicator" status="on"/> When the far end destination goes on-hook, CM notifies the same via <feature name ="busy-indicator" status="off"/>
CSFeatureTypeAutodial | Autodial is a feature button which can be configured as a speed-dial either by Admin or the user. User can edit the autodial Label and/or number. User can always edit the destinationLabel User can edit the destinationExtension if the isDestinationExtensionEditable flag is true.
CSFeatureTypeHuntGroupBusyPosition | Hunt Group Busy Position is a feature button which allows user to opt-in/opt-out from Hunt Group calls. If your admin have configured your extension as a member of a hunt group, you will be eligible to receive calls made to that hunt group. When you don't want to receive calls on that hunt group, the feature needs to be enabled. When feature is enabled, user will not receive any calls on that Hunt Group. When feature is disabled, user will start recieving the calls on that hunt group again. User can also set the personalized label for the button.
CSFeatureTypeTeamButton | The Team Button feature allows the user to view the state of another station and allow the user to answer any calls which are actively ringing on that station. The button can also be used as a speed dial to call the monitored station when it is idle.
CSFeatureTypeMaliciousCallTrace | Malicious Call Trace (MCT) feature lets a user to notify SM about a malicious call when a user invokes the Malicious Call Trace feature on an incoming call.
CSFeatureTypeNoHoldConference | The No Hold Conference feature allows a user to set up a conference call without interrupting the current conversation. The called party is automatically added to the conference as soon as they answer.
CSFeatureTypeLimitCalls | Limit Number of Concurrent Calls feature: Users can use this to limit the number of concurrent calls at a station to one call, where normally multiple call appearances can terminate at the station.
CSFeatureTypeServiceObserving | The Service Observing (SO) features allow a supervisor or other authorized user to use their telephone to activate an observing session towards a station, an agent LoginID or VDN to listen in and possibly talk on calls received by the station/agent or VDN for the purposes of quality control and training.
CSFeatureTypeForwardBusyCall | This feature enables forwarding when the user's extension is busy. It uses the Forward Number destination or, if set, the Forward on Busy Number destination. If the user has call appearance buttons programmed, the system will not treat them as busy until all the call appearance buttons are in use. Note that this feature differs from the feature FORWARD_BUSY_NO_ANSWER_CALLS since the latter one serves invocation of both busy and not answered cases (for platforms where the two cases can not be supported separately).
CSFeatureTypeForwardNoAnswerCalls | This feature enables forwarding when the user's extension is not answered within the period defined by their No Answer Time. It uses the Forward Number destination or, if set, the Forward on Busy Number destination. Note that this feature differs from the feature FORWARD_BUSY_NO_ANSWER_CALLS since the latter one serves invocation of both busy and not answered cases (for platforms where the two cases can not be supported separately).
CSFeatureTypeForwardNumber | This feature sets the number to which the user's calls are redirected. This can be an internal or external number. This feature does not activate forwarding; it only sets the number for the forwarding destination. This number is used for all forward types; Forward Unconditional, Forward on Busy and Forward on No Answer, unless the user has a separate Forward on Busy Number set for forward on busy and forward on no answer functions.
CSFeatureTypeForwardBusyNumber | This feature sets the number to which the user's calls are forwarded when Forward on Busy or Forward on No Answer are on. If no Forward on Busy Number is set, those functions use the Forward Number. This feature does not activate the forwarding, it only sets the number for the forwarding destination.
CSFeatureTypeAutoConference | This feature can be used to place the user, his current call and any calls he has on hold into a conference. If the call on hold is an existing conference, the user and any current call are added to that conference.
CSFeatureTypeCancelAllForwarding | This feature cancels all forms of forwarding on the user's extension including "Follow Me" and "Do Not Disturb".
CSFeatureTypeForwardToVoiceMail | This feature allows the user to define voicemail box usage. When feature is enabled: the user's voicemail mailbox is used to answer calls which ring unanswered or arrive when the user is busy. When feature is disabled: the user's voicemail mailbox box is not being used to answer calls. This does not disable the voicemail mailbox being used as the target for other functions such as call recording or messages forwarded from other mailboxes.
CSFeatureTypeStationLogout | This feature logs the user off the phone or soft client he is currently logged in. Results in regular logout process for the environments/platforms which do not let the user to logout without this feature assigned.
CSFeatureTypeDirectDial | This feature allows to call an extension and have the call automatically answered on speaker phone after 3 beeps. The called extension must support a handsfree speaker. If the extension does not have a handsfree microphone then the user must use the handset if he wants to talk. If the extension is not free when called, the call is presented as a normal call on a call appearance button if available.
CSFeatureTypeMoveCall | This feature allows the user to move the active call to either a simultaneous client or twinned destination.
CSFeatureTypeRetrieveCall | This feature allows the user to retrieve the active call from either a simultaneous client or twinned destination.
CSFeatureTypeInternalTwinning | When this feature is active, incoming calls will ring on the user's own extension and another extension within the same IP Office. This feature can only be configured by the IP Office administrator. User will not be able to activate/deactivate this feature.
CSFeatureTypeSimRingCallback | This feature allows to configure parameters for simultaneous ringing on incoming calls and/or originating callback call.
CSFeatureTypeCallbackCall | This feature allows the user to configure callback call from the given caller destination to the remote destination.
CSFeatureTypeSendNN | Send-NN ( Send number and name ), this feature allows to place outgoing calls while hiding or replacing the caller's number/identity with the specified caller number or identity.