Avaya Client Services API Reference (iOS)

- Main Page
- Classes
- Files
- Related Pages

- File List
- File Members

Enumerations
CSMediaTransportPreference.h File Reference
`#import <Foundation/Foundation.h>`

## Enumerations
enum | CSMediaTransportPreference { CSMediaTransportNoMedia = 0, CSMediaTransportAllTransports, CSMediaTransportWifiOnly, CSMediaTransportCellular }
| The list of Media Transport network preferences. More...

## Enumeration Type Documentation

enum CSMediaTransportPreference

The list of Media Transport network preferences.

This structure provides a list of choices based on the network type preference. A feature (i.e. VoIP calls, or video) can be enabled based on network connectivity. It is necessary to allow a feature to be enabled based on the preference of network connectivity. All Transports (enabled) and No Media (disabled are independent of network type. The WiFI only state is included to indicate that the feature is dependent on WiFi connectivity.

Enumerator
CSMediaTransportNoMedia |
CSMediaTransportAllTransports |
CSMediaTransportWifiOnly |
CSMediaTransportCellular | Indicates user’s preference to use cellular network for telephony features and media. When both WiFi and cellular data network connectivity are available, SIP-based telephony signaling and media traffic are routed through the cellular data network. HTTP-based telephony and media traffic are routed through WiFi. When cellular data network connectivity is not available but WiFi connectivity is, all telephony and media traffic are routed through WiFi. If cellular data network connectivity becomes available while connected through WiFi, SIP-based signaling and any active SIP-based call(s) will be moved over to the cellular data network.