Avaya Client Services API Reference (Windows)
Avaya Client Services API Reference (Windows)
Avaya.ClientServices
AudioDetails Class
AudioDetails Properties
AverageLocalJitterMilliseconds Property
AverageRemoteJitterMilliseconds Property
BytesReceived Property
BytesTransmitted Property
Codec Property
CurrentAccelerateRate Property
CurrentBufferSizeMilliseconds Property
CurrentDiscardRate Property
CurrentExpandRate Property
CurrentPacketLossRate Property
CurrentPreemptiveRate Property
DtmfPayloadType Property
EncryptionType Property
IsMediaProxied Property
IsMediaTunneled Property
LocalFractionLost Property
LocalIPAddress Property
LocalPort Property
PacketizationMilliseconds Property
PacketsReceived Property
PacketsTransmitted Property
PreferredBufferSizeMilliseconds Property
RemoteFractionLost Property
RemoteIPAddress Property
RemotePort Property
RoundTripTimeMilliseconds Property
RtcpEncrypted Property

# AudioDetails Properties

The AudioDetails type exposes the following members.

Properties

| Name | Description
--- | --- | ---
| AverageLocalJitterMilliseconds | The average jitter buffer size (in milliseconds) the local end is experiencing on the received RTP stream.
| AverageRemoteJitterMilliseconds | The average jitter buffer size (in milliseconds) the remote end is experiencing on the transmitted RTP stream.
| BytesReceived | The total number of RTP payload bytes received.
| BytesTransmitted | The total number of RTP payload bytes transmitted.
| Codec | The name of the audio codec being used.
| CurrentAccelerateRate | The fraction of data removed through acceleration.
| CurrentBufferSizeMilliseconds | The current jitter buffer size in milliseconds.
| CurrentDiscardRate | The percentage of packets discarded (late).
| CurrentExpandRate | The fraction of synthesized speech frames inserted through expansion in total frame count in buffer.
| CurrentPacketLossRate | The percentage of packets lost (network + late).
| CurrentPreemptiveRate | The fraction of synthesized speech frames inserted through pre-emptive expansion in total frame count in buffer.
| DtmfPayloadType | The dynamic payload type used for telephony events (DTMF tones).
| EncryptionType | Media encryption type.
| IsMediaProxied | Status indication for whether tunneled Audio goes through proxy or not.
| IsMediaTunneled | Status indication for whether Audio tunneled or not.
| LocalFractionLost | The fractional loss seen locally.
| LocalIPAddress | The local IP address used for the audio session.
| LocalPort | The local RTP receive port for the audio session (as per SDP offer/answer exchange).
| PacketizationMilliseconds | The packetization interval in milliseconds.
| PacketsReceived | The total number of RTP packets received.
| PacketsTransmitted | The total number of RTP packets transmitted.
| PreferredBufferSizeMilliseconds | The preferred (optimal) jitter buffer size in milliseconds.
| RemoteFractionLost | The fractional loss seen remotely which far end sends to local end through RTCP.
| RemoteIPAddress | The remote IP address used for the audio session.
| RemotePort | The remote RTP receive port for the audio session (as per SDP offer/answer exchange).
| RoundTripTimeMilliseconds | The round-trip audio delay (in milliseconds) calculated as per RFC 3550.
| RtcpEncrypted | Indicates whether RTCP is encrypted or not. True if feedback RTCP packets are encrypted false otherwise. If it is true RTCP packets should be decrypted before reading audio stream details.

Top
See Also

#### Reference

AudioDetails Class
Avaya.ClientServices Namespace

© 2017 Avaya LLC. All Rights Reserved.