Avaya Client Services API Reference (Windows)
Avaya Client Services API Reference (Windows)
Avaya.ClientServices
SignalingPingConfiguration Class
SignalingPingConfiguration Properties
TcpKeepAliveEnabled Property
TcpKeepAliveIntervalInSeconds Property
TcpKeepAliveRetryIntervalInSeconds Property

# SignalingPingConfiguration Properties

The SignalingPingConfiguration type exposes the following members.

Properties

| Name | Description
--- | --- | ---
| TcpKeepAliveEnabled | Specifies whether or not the telephone sends TCP keep alive messages.
| TcpKeepAliveIntervalInSeconds | Specifies the number of seconds that the telephone will wait before sending out a TCP keep-alive (TCP ACK) message. Valid values are 10 through 3600. Default is 60 seconds.
| TcpKeepAliveRetryIntervalInSeconds | Specifies the number of seconds that the telephone will wait before re-transmitting a TCP keep-alive (TCP ACK) message. Valid values are 5 through 60. Default is 10 seconds

Top
See Also

#### Reference

SignalingPingConfiguration Class
Avaya.ClientServices Namespace

© 2017 Avaya LLC. All Rights Reserved.