Avaya Client Services API Reference (Windows)
Avaya Client Services API Reference (Windows)
Avaya.ClientServices
SignalingPingConfiguration Class
SignalingPingConfiguration Properties
TcpKeepAliveEnabled Property
TcpKeepAliveIntervalInSeconds Property
TcpKeepAliveRetryIntervalInSeconds Property

SignalingPingConfiguration Properties

The SignalingPingConfiguration type exposes the following members.

Properties

| Name | Description
--- | --- | ---
| TcpKeepAliveEnabled | Specifies whether or not the telephone sends TCP keep alive messages.
| TcpKeepAliveIntervalInSeconds | Specifies the number of seconds that the telephone will wait before sending out a TCP keep-alive (TCP ACK) message. Valid values are 10 through 3600. Default is 60 seconds.
| TcpKeepAliveRetryIntervalInSeconds | Specifies the number of seconds that the telephone will wait before re-transmitting a TCP keep-alive (TCP ACK) message. Valid values are 5 through 60. Default is 10 seconds

Top
See Also

#### Reference

SignalingPingConfiguration Class
Avaya.ClientServices Namespace

© 2017 Avaya LLC. All Rights Reserved.