Avaya Client Services API Reference (Windows)
Avaya Client Services API Reference (Windows)
Avaya.ClientServices
SipUserConfiguration Class
SipUserConfiguration Properties
AutomaticLineReservationEnabled Property
BlindTransferEnabled Property
CallDenialPolicy Property
ConnectionPolicy Property
CredentialProvider Property
DialPlan Property
DisplayName Property
Domain Property
EmergencyNumbers Property
EmergencyNumbersOrdered Property
EnableAlternateCLI Property
EnableAsControlledEndpoint Property
Enabled Property
EnableDeskphoneModeOnStartup Property
EnableMacAddressInfoInSIPRegistration Property
InitiateTCCallWhenForwardingEnabled Property
Language Property
MaxNumberOfControllingEndpoints Property
MaxSimultaneousRegistrations Property
MediaAddressMode Property
MediaEncryptionTypeArray Property
OtherPhoneModeRemoteMediaResponseTimeout Property
OutboundSubscriptionConfiguration Property
PreferredContactURI Property
PreserveDialogsOnFailover Property
RTCP5TracerouteCollectionEnabled Property
SignalingAddressMode Property
SipAgentConfiguration Property
SipClientConfiguration Property
SrtcpEnabled Property
SRTPRekeyingOnUnholdEnabled Property
TransferToVoicemailEnabled Property
UserId Property
UserToUserInformationEnabled Property
UseSIPSURIOverTLS Property
VoIPCallingPreference Property

SipUserConfiguration EnableMacAddressInfoInSIPRegistration Property

Controls whether the local MAC address information is passed in the SIP registration message.

Namespace: Avaya.ClientServices
Assembly: AvayaClientServices (in AvayaClientServices.dll) Version: 592.1.30.0
Syntax
C#
Copy

    public bool EnableMacAddressInfoInSIPRegistration { get; set; }

#### Property Value

Type: Boolean
Remarks
Controls whether the local MAC address information is provided in the "+av.mac-address" field of the SIP registration contact address or not. By default, this property is set to false, indicating that no local MAC address information is provided in the SIP registration message. When this property is set to true and the local operating system allows reading of the MAC address based on the local IP address used for connection to the SIP server, then the local MAC address is provided in the "+av.mac-address" field. The MAC address provided in the "+av.mac-address" field is used by Avaya development partners to determine the location of the machine for E.911 calling.
See Also

#### Reference

SipUserConfiguration Class
Avaya.ClientServices Namespace

© 2017 Avaya LLC. All Rights Reserved.