Avaya Client Services API Reference (Windows)
Avaya Client Services API Reference (Windows)
Avaya.ClientServices
HttpUserConfiguration Class
HttpUserConfiguration Properties
Enabled Property
HttpClientConfiguration Property
MediaAddressMode Property
MediaEncryptionTypeArray Property
MediaTunnelingEnabled Property
MediaTunnelingEnforced Property
SrtcpEnabled Property
VoIPCallingPreference Property

# HttpUserConfiguration MediaAddressMode Property

Indicates the IP address type preference to use while transporting media for HTTP calls from a dual stack client network. Currently IPv4 and IPv6 are the valid options supported by Client SDK. IPv4Then6 and IPv6Then4 are internally treated as IPv4 and IPv6 respectively for HTTP calls.

Namespace: Avaya.ClientServices
Assembly: AvayaClientServices (in AvayaClientServices.dll) Version: 550.0.60.0
Syntax
C#
Copy

    public MediaAddressMode MediaAddressMode { get; set; }

#### Property Value

Type: MediaAddressMode
See Also

#### Reference

HttpUserConfiguration Class
Avaya.ClientServices Namespace

© 2017 Avaya LLC. All Rights Reserved.