Avaya Client Services API Reference (Windows)
Avaya Client Services API Reference (Windows)
Avaya.ClientServices
SignalingPingConfiguration Class
SignalingPingConfiguration Properties
TcpKeepAliveEnabled Property
TcpKeepAliveIntervalInSeconds Property
TcpKeepAliveRetryIntervalInSeconds Property

# SignalingPingConfiguration TcpKeepAliveIntervalInSeconds Property

Specifies the number of seconds that the telephone will wait before sending out a TCP keep-alive (TCP ACK) message. Valid values are 10 through 3600. Default is 60 seconds.

Namespace: Avaya.ClientServices
Assembly: AvayaClientServices (in AvayaClientServices.dll) Version: 550.0.60.0
Syntax
C#
Copy

    public int TcpKeepAliveIntervalInSeconds { get; set; }

#### Property Value

Type: Int32
See Also

#### Reference

SignalingPingConfiguration Class
Avaya.ClientServices Namespace

© 2017 Avaya LLC. All Rights Reserved.