Avaya Client Services API Reference (Windows)
Avaya Client Services API Reference (Windows)
Avaya.ClientServices
SignalingPingConfiguration Class
SignalingPingConfiguration Properties
TcpKeepAliveEnabled Property
TcpKeepAliveIntervalInSeconds Property
TcpKeepAliveRetryIntervalInSeconds Property

# SignalingPingConfiguration TcpKeepAliveRetryIntervalInSeconds Property

Specifies the number of seconds that the telephone will wait before re-transmitting a TCP keep-alive (TCP ACK) message. Valid values are 5 through 60. Default is 10 seconds

Namespace: Avaya.ClientServices
Assembly: AvayaClientServices (in AvayaClientServices.dll) Version: 550.0.60.0
Syntax
C#
Copy

    public int TcpKeepAliveRetryIntervalInSeconds { get; set; }

#### Property Value

Type: Int32
See Also

#### Reference

SignalingPingConfiguration Class
Avaya.ClientServices Namespace

© 2017 Avaya LLC. All Rights Reserved.