Avaya Client Services API Reference (Windows)
Avaya Client Services API Reference (Windows)
Avaya.ClientServices
SignalingPingConfiguration Class
SignalingPingConfiguration Properties
TcpKeepAliveEnabled Property
TcpKeepAliveIntervalInSeconds Property
TcpKeepAliveRetryIntervalInSeconds Property

SignalingPingConfiguration TcpKeepAliveIntervalInSeconds Property

Specifies the number of seconds that the telephone will wait before sending out a TCP keep-alive (TCP ACK) message. Valid values are 10 through 3600. Default is 60 seconds.

Namespace: Avaya.ClientServices
Assembly: AvayaClientServices (in AvayaClientServices.dll) Version: 592.1.30.0
Syntax
C#
Copy

    public int TcpKeepAliveIntervalInSeconds { get; set; }

#### Property Value

Type: Int32
See Also

#### Reference

SignalingPingConfiguration Class
Avaya.ClientServices Namespace

© 2017 Avaya LLC. All Rights Reserved.