Avaya Client Services API Reference (Windows)
Avaya Client Services API Reference (Windows)
Avaya.ClientServices
SipUserConfiguration Class
SipUserConfiguration Properties
AutomaticLineReservationEnabled Property
BlindTransferEnabled Property
CallDenialPolicy Property
ConnectionPolicy Property
CredentialProvider Property
DialPlan Property
DisplayName Property
Domain Property
EmergencyNumbers Property
EmergencyNumbersOrdered Property
EnableAlternateCLI Property
EnableAsControlledEndpoint Property
Enabled Property
EnableDeskphoneModeOnStartup Property
EnableMacAddressInfoInSIPRegistration Property
InitiateTCCallWhenForwardingEnabled Property
Language Property
MaxNumberOfControllingEndpoints Property
MaxSimultaneousRegistrations Property
MediaAddressMode Property
MediaEncryptionTypeArray Property
OtherPhoneModeRemoteMediaResponseTimeout Property
OutboundSubscriptionConfiguration Property
PreferredContactURI Property
PreserveDialogsOnFailover Property
RTCP5TracerouteCollectionEnabled Property
SignalingAddressMode Property
SipAgentConfiguration Property
SipClientConfiguration Property
SrtcpEnabled Property
SRTPRekeyingOnUnholdEnabled Property
TransferToVoicemailEnabled Property
UserId Property
UserToUserInformationEnabled Property
UseSIPSURIOverTLS Property
VoIPCallingPreference Property

SipUserConfiguration InitiateTCCallWhenForwardingEnabled Property

When Send All Calls feature is enabled, there continues to be an incoming call notification that arrives at the client application, and will be forwarded to the Telecommuter device and cancelled when the Aura coverage timer fires. To avoid the unnecessary signalling, the property may be set to disable.

Namespace: Avaya.ClientServices
Assembly: AvayaClientServices (in AvayaClientServices.dll) Version: 592.1.30.0
Syntax
C#
Copy

    public bool InitiateTCCallWhenForwardingEnabled { get; set; }

#### Property Value

Type: Boolean
Remarks
If enabled, the SIP endpoint starts a call on Telecommuter leg. If disabled, the SIP endpoint doesn't relay incoming INVITE and doesn't start a call on Telecommuter leg.
See Also

#### Reference

SipUserConfiguration Class
Avaya.ClientServices Namespace

© 2017 Avaya LLC. All Rights Reserved.